「공내 카메라장비 구입」 규격서

1. 건    명

□ 2020년 지하수 관측시설 유지관리 사업 「공내 카메라장비 구입」

2. 구입내역

□ 공내카메라장비 - 1세트

• 윈치(Deluxe Electric Winch)	1대

• 카메라(Dual-Scan Micro Camera)	2개

□ 부대 장비

• Depth encoder for screen         1개

• Cable End Replacement kit       1개

• 7-inch LCD모니터	1개

• 인버터	1개

3. 구입조건

○ 발주기관이 지정하는 장소에 납품하고, 발주기관의 검수자 입회하에 계측자료의 신뢰도 검증 및 정상작동 여부 확인, 사용자 교육을 실시하여야 한다.

○ 납품은 계약일로부터 60일 이내에 완료하여야 하며, 이 기간 내에 현장시험 및 사용자 교육을 실시하여야 한다.

○ 보증기간은 납품완료일로부터 1년간으로 하고, 보증기간 중 A/S요청이 있을 때에는 즉시 응해야 하며, 수리부품 및 경비는 도급자가 부담한다.

○ 납품 시 제조사의 품질보증서 및 시험성적서, 사용설명서를 제출하여야 한다.

4. 세부규격 및 사양

□ 공내카메라장비

품 명	사 양
윈치(전기 방식)	- Input Voltage: 120VAC or 240VAC @50-60Hz
	- Cable length: 600 meters
	- Weights: 96 lbs (44kg)
	- Output Voltage: 12-48 VDC
	- Dimensions: 24" x 24" x 19" (61 cm x 61 cm x 48 cm)
	- Depth encoder for screen
카메라 (Dual-Scan Micro Camera)	- Weight: 3.5 lb (1.59 kg)
	- Dimensions: 27" long × 1-1/8" diameter (68.6 cm × 2.9 cm)
	- CCD: 1/3" Sony Super HAD CCD II
	- Standard lens: 2.45 mm Down-Looking, 2.97 mm Side-Looking
	- Angle of View (in air): ~150° Down-Looking, ~130° Side-Looking
	- Aperture: F2.0
	- Video Format: NTSC
	- Aspect Ratio: 4:3
	- Horizontal Resolution: 550 LInes
	- Effective Pixels: 768 Horizontal x 494 Vertical
	- Light Source: 9-9-3 High Intensity White LEDs
	- Operating Temperature: -40 °F ~ 122 °F (-40 °C ~ 50 °C)
	- Maximum Pressure: 1000 psi
	- Maximum Depth: 600 meters
	- Window Meterial: Sapphire
	- Exposure Control: Yes - Both cameras

5. 부대 장비

□ 7-inch LCD모니터	1개

□ 인버터	1개

□ Depth encoder for screen         1개

□ Cable End Replacement kit       1개

품 명	사 양
7-inch LCD 모니터	- Screen Size: 7 inch
	- System: NTSC
	- Display Method: TFT Active matrix system
	- Resolution: 1440 x 234
인버터	- Continuous Output Power: 300 Watts
	- Peak Output Power: 500 Watts
	- Frequency: 60 hz
	- Input Voltage: 12 VDC
	- Output Voltage: 120 VAC
	- Dimension: 8.5" x 5.8" x 2.6" (215 x 147 x 66 mm)
	- Weight: 2.9 lb (1.3 kg)